Round turn and two half-hitches

This is a long name for a simple hitch used to attach a rope to a post, spar, tree, and so on. It

is a composite knot formed from two simple knots.

· Form a round turn by turning the working end twice around the post.
· Then form a half-hitch by taking the working end around the standing part forming a crossed loop.

· Repeat to form a second half-hitch. These should be tied in the same direction and tightened up against the post to ensure that the round turn doesn't slip.
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